|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-19) Sharm el-Sheikh, Egypt, 28 October – 22 November 2019** |  |
|  |  |
|  | CPG(19)101 ANNEX VIII-19KR1 |
| PLENARY MEETING | **Addendum 11 to**  **Addendum 19 to Document XXX-E** |
|  | **Date** |
|  | **Original: English** |
|  | |
| European Common Proposals | |
| Proposals for the work of the conference | |
|  | |
| Agenda item 7(K) | |

7 to consider possible changes, and other options, in response to Resolution 86 (Rev. Marrakesh, 2002) of the Plenipotentiary Conference, an advance publication, coordination, notification and recording procedures for frequency assignments pertaining to satellite networks, in accordance with Resolution **86 (Rev.WRC-07)**, in order to facilitate rational, efficient and economical use of radio frequencies and any associated orbits, including the geostationary-satellite orbit;

7(K) Issue K - Difficulties for Part B examinations under § 4.1.12 or 4.2.16 of RR Appendices **30** and **30A** and § 6.21 c) of RR Appendix **30B**

Introduction

To address the difficulties encountered by the notifying administration in the Part B examination of its junior network under § 4.1.12 or § 4.2.16 of RR Appendices **30** and**30A** or § 6.21 *c)* of RR Appendix **30B**, it is proposed to add one more examination under § 4.1.12 or § 4.2.16 of RR Appendices **30** and **30A** and § 6.21 *c)* of RR Appendix **30B** such that should any remaining affected networks whose assignments have been entered in the List or Plan, as appropriate, before the submission under § 4.1.12 or § 4.2.16 of RR Appendices **30** and **30A** or § 6.17 of RR Appendix **30B**, the Bureau shall further examine if the remaining corresponding assignments in the List or Plan are still considered as being affected.

In this way, like the current practice today, if examination under § 4.1.12 or § 4.2.16 of RR Appendices **30** and **30A** or § 6.21 *c)* of RR Appendix **30B** of Part B of a junior network in respect of Part A of a senior network is favourable, the senior network is considered as not being affected like today and no further examination will be conducted.

Meanwhile, it addresses the difficulties experienced by the notifying administration and allows its Part B notice submitted under § 4.1.12 or § 4.2.16 of RR Appendices **30** and **30A** or § 6.17 of RR Appendix **30B** to receive favourable findings in respect of senior network if its Part B is considered as not affected in the further examination based on the method of Annex 1 (RR Appendix **30**), Annex 1 (RR Appendix **30A**) or Annex 4 (RR Appendix **30B**). This avoids overprotection of senior networks based on the characteristics which are outdated and no longer valid while ensuring that senior networks are adequately protected.

In the European view, this procedure will better reflect the actual situation and enable newcomers to benefit from the reduction of satellite networks parameters and characteristics of other networks emerging during the coordination process, and thus increase the efficiency of spectrum use. This method corresponds to the single method in the CPM Report.

Proposals

APPENDIX 30 (REV.WRC‑15)\*

Provisions for all services and associated Plans and List1 for  
the broadcasting-satellite service in the frequency bands  
11.7-12.2 GHz (in Region 3), 11.7-12.5 GHz (in Region 1)  
         and 12.2-12.7 GHz (in Region 2)    (WRC‑03)

ARTICLE 4     (Rev.WRC‑15)

Procedures for modifications to the Region 2 Plan or   
for additional uses in Regions 1 and 33

## 4.1 Provisions applicable to Regions 1 and 3

MOD EUR/XXXA19A11/1

4.1.12 [[1]](#footnote-1)XX If agreement has been reached with the administrations identified in the publication referred to under § 4.1.5 above, the administration proposing the new or modified assignment may continue with the appropriate procedure in Article 5, and shall so inform the Bureau, indicating the final characteristics of the frequency assignment together with the names of the administrations with which agreement has been reached.     (WRC‑19)

**Reasons:** To better reflect the actual situation and enable newcomers to benefit from the reduction of satellite networks parameters and characteristics of other networks emerging during the coordination process, and thus increase the efficiency of spectrum use.

## 4.2 Provisions applicable to Region 2

MOD EUR/XXXXA19A11/2

4.2.16 [[2]](#footnote-2)XX1 If no comments have been received on the expiry of the periods specified in § 4.2.14, or if agreement has been reached with the administrations which have made comments and with which agreement is necessary, the administration proposing the modification may continue with the appropriate procedure in Article 5, and shall so inform the Bureau, indicating the final characteristics of the frequency assignment together with the names of the administrations with which agreement has been reached.     (WRC‑19)

APPENDIX 30A (REV.WRC‑15)\*

Provisions and associated Plans and List1 for feeder links for the broadcasting-satellite service (11.7-12.5 GHz in Region 1, 12.2-12.7 GHz  
in Region 2 and 11.7-12.2 GHz in Region 3) in the frequency bands  
14.5-14.8 GHz2 and 17.3-18.1 GHz in Regions 1 and 3,  
and 17.3-17.8 GHz in Region 2     (WRC‑03)

ARTICLE 4     (Rev.WRC‑15)

Procedures for modifications to the Region 2 feeder-link Plan   
or for additional uses in Regions 1 and 3

## 4.1 Provisions applicable to Regions 1 and 3

MOD EUR/XXXXA19A11/3

4.1.12 [[3]](#footnote-3)XX If agreement has been reached with the administrations identified in the publication referred to under § 4.1.5 above, the administration proposing the new or modified assignment may continue with the appropriate procedure in Article 5 and shall inform the Bureau, indicating the final characteristics of the frequency assignment together with the names of the administrations with which agreement has been reached.      (WRC-19)

## 4.2 Provisions applicable to Region 2

MOD EUR/XXXXA19A11/4

4.2.16 [[4]](#footnote-4)XX1 If no comments have been received on the expiry of the periods specified in § 4.2.14, or if agreement has been reached with the administrations which have made comments and with which agreement is necessary, the administration proposing the modification may continue with the appropriate procedure in Article 5, and shall so inform the Bureau, indicating the final characteristics of the frequency assignment together with the names of the administrations with which agreement has been reached.     (WRC‑19)

APPENDIX 30B (REV.WRC‑15)

Provisions and associated Plan for the fixed-satellite service  
in the frequency bands 4 500-4 800 MHz, 6 725-7 025 MHz,  
10.70-10.95 GHz, 11.20-11.45 GHz and 12.75-13.25 GHz

ARTICLE 6     (REV.WRC‑15)

Procedures for the conversion of an allotment into an assignment, for  
the introduction of an additional system or for the modification of  
an assignment in the List1, 2     (WRC‑15)

MOD EUR/XXXA19A11/5

6.21 When the examination with respect to § 6.19 of an assignment received under § 6.17 leads to a favourable finding, the Bureau shall use the method of Annex 4 to examine if the affected administrations and the corresponding:

*a)* allotments in the Plan;

*b)* assignments which appear in the List at the date of receipt of the examined notice submitted under § 6.1;

*c)* assignments for which the Bureau has previously received complete information in accordance with § 6.1 and has conducted the examination under § 6.5 of this Article at the date of receipt of the examined notice submitted EMP [[5]](#footnote-5)YY;

indicated in the Special Section published under § 6.7 and whose agreement has not been provided under § 6.17 are still considered as being affected by that assignment.     (WRC‑19)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. XX Should any remaining affected networks whose assignments have been entered in the List before the notice received under § 4.1.12, the Bureau shall use the method of Annex 1 to further examine if the remaining corresponding assignments in the List are still considered as being affected. The examination in respect of those remaining affected networks is conducted independently using the Appendices **30** and **30A** master database corresponding to the Part B Special Section that was published under § 4.1.15. Resolution **548 (Rev.WRC‑12)** applies.      (WRC‑19) [↑](#footnote-ref-1)
2. XX1 Should any remaining affected networks whose assignments have been entered in the Plan before the notice received under § 4.2.16, the Bureau shall use the method of Annex 1 to further examine if the remaining corresponding assignments in the Plan are still considered as being affected. The examination in respect of those remaining affected networks is conducted independently using the Appendices **30** and **30A** master database corresponding to the Part B Special Section that was published under § 4.2.19.      (WRC‑19) [↑](#footnote-ref-2)
3. XX Should any remaining affected networks whose assignments have been entered in the List before the notice received under § 4.1.12, the Bureau shall use the method of Annex 1 to further examine if the remaining corresponding assignments in the List are still considered as being affected. The examination in respect of those remaining affected networks is conducted independently using the Appendices **30** and **30A** master database corresponding to the Part B Special Section that was published under § 4.1.15. Resolution **548 (Rev.WRC‑12)** applies.      (WRC‑19) [↑](#footnote-ref-3)
4. XX1 Should any remaining affected networks whose assignments have been entered in the Plan before the notice received under § 4.2.16, the Bureau shall use the method of Annex 1 to further examine if the remaining corresponding assignments in the Plan are still considered as being affected. The examination in respect of those remaining affected networks is conducted independently using the Appendices **30** and **30A** master database corresponding to the Part B Special Section that was published under § 4.2.19.      (WRC‑19) [↑](#footnote-ref-4)
5. YY Should any remaining affected networks whose assignments have been entered in the List before the notice received under § 6.17, the Bureau shall use the method of Annex 4 to further examine if the remaining corresponding assignments in the List are still considered as being affected. The examination in respect of those remaining affected networks is conducted independently using the Appendix **30B** master database corresponding to the A6B Special Section that was published under § 6.23 or § 6.25.      (WRC‑19) [↑](#footnote-ref-5)